# Summary of Argyll CMS Changes since last release

### For a complete and more detailed list of changes, please see the log.txt file.

# [V2.1.2 -> V2.2.0] 3rd May 2021

- Added native i1Pro3 and i1Pro3 Plus driver.
- Fix Apple M1 display name code & builds. (Thanks to Simone Karin). Should work now using Rosetta 2 or as M1 native binaries.
- Fix bug in applycal.c where it gets an "Error - Write file: 1, icmTextDescription_write: ascii string is shorter" error on replacing one calibration with another.
- Improved i1pro & Munki patch recognition to work much more reliably with a slow swipe speed.
- Fixed oeminst to work with spyder V5.5. setup.exe
- Fixed bug in oemdld that prevented HTML encoded characters in download file decoding properly, which prevented certain filenames from working.
- Fixed bug in ccxxmake -S -f where save error wasn't being fully reported, and display technology presence check was faulty.
- Fixed typo in display technology, VPA -> PVA.
- Made Klein K10A "Lights Off" command timeout a soft error. For some reason this command doesn't seem to be implemented on some K10A's.
- Fixed OS X 10.15 compatibility problem with change in objc_msgSend declaration. (Thanks to Misty De Meo)
- Added CIE dE2000 to spotread output.
- Fixed accidental global "wrl" in gamut/gamut.h that cases compile warnings.

# [V2.1.1 -> V2.1.2] 14th January 2020

- Added -d option to spotread to print out Density values.
- Improved i1Pro2 emissive measurement compatibility with X-Rite driver.
- Changed targen round down/up to 0%/100% to have a tighter tolerance.
- Added -Yk flag to spectro/dispread, to restore a workflow in which display calibration is done without using vcgt hardware.
- Modified txt2ti3 to cope with files that don't have SampleName/SampleID fields, such as CoPrA sample files.
- Added instrument ambient mode (-a flag) to dispcal, dispread and ccxxmake, to allow use of direct projector to ambient mode measurement.
- Fixed problem with i1Pro2 EO2-XR-UF model crashing when high-res mode used.
- Changed dispcal ADJ_THRESH mode MIN_THRESH value to 0.25 from 0.05, as well as restricting it to the last pass, to reduce pointless repeats of dark values.

# [V2.1.0 -> V2.1.1] 29th April 2019

- Fix typo in usb/55-Argyll.rules for i1Studio.
- Added SpyderX support for inst_opt_noinitcalib option, so that the -N flag can be honoured. (Thanks to Florian Hoch)

# [V2.0.1 -> V2.1.0] 10th April 2019

- Added scanin .cht for Christophe Metairie's Digital Target 2019 and Digital Target Studio Edition input charts.
- Added support for Lasersoft ISO12641-2 reflective and 3 part transmissive charts (recognition files, cxf2ti3 tool, changes to average utility).
- Changed spotread -E option to work with all the spectral instruments, and now argument should be a transmission spectrum of the filter placed on the instrument.
- Added targen options -M to generate device space cube surface steps, and -n option to generate neutral axis steps based on a pre-conditioning profile.
- Added support for SpyderX colorimeter.
- Improvements and bug fixes to oeminst and oemdnld.
- Add IES TM-30-15 (Method for Evaluating Light Source Color Rendition) to spotread.
- Added optional spectrum save file argument to spotread -O option.
- Changed spotread so that plot option -S doesn't wait for a keystroke before continuing.
- Fix FWA bugs in spotread - wasn't saving FWA compensated spectra, was double correcting reference spectra.
- Changed colprof Display profile -ax option to create just XYZ cLUT profiles, rather than including dummy channel swapped matrix as well. This will force the use of the cLUT tags in any application/CMM that uses an unconventional tag priority when dealing with a profile that contains both cLUT and shaper/matrix tags. The -aY option has been added to create a diagnostic cLUT display profile that contains matrix tags with swapped color channels.
- Change black ink "locus" rules (i.e. -K option) to just scale from zero to maximum possible K, rather than minimum to maximum K. This makes these rules much more usable, since the sharp increase in minimum black near the black point will no longer badly distort the curve shape. This affects colprof, collink and xicclu.

# [V2.0.0 -> V2.0.1] 9th July 2018

- Increased maximum render channels to 16
- Added -O option to collink to allow creating a link purely from calibration file.
- Fixed JETI specbos & specval timeout when in averaging mode and dark measurement.
- Changed JETI specval 1511 driver to ignore REMOTE command error with newer firmware.
- Changed Klein K10 serial parameters in attempt to prevent serial lock up on MSWindows.
- Made a failure of the conf:maxtin command with a JETI 1201 a soft error, to allow for old firmware versions.
- Change colorhug Linux driver to reset on close. This may overcome a problem re-starting the driver.
- Fixed i1Pro driver to cope with stripped down OEM i1Pro2 that is missing one piece of calibration information.
- Fixed display calibration selection to allow for more than 62 entries. This is to fix problem using Klein K10 that has a lot of saved calibrations.
- Changed spec2cie to add extra informational L*a*b* output fields, if a non D50 illuminant (-i option) is used.
- Added -w parameter to spotread, to use the -i parameter illuminant for L*a*b* calculation.
- Fixed bug in spec2cie - XRGA conversion wasn't saving spectrum out.

# [V1.9.2 -> V2.0.0] 17th November 2017

- Added support for "pm" viewing condition (Print evaluation with partial Mid-tone adaptation), and associated m: viewing condition parameter. This is intended to address certain situations involving the use of papers containing FWA/OBE brighteners when viewed in an environment that has a very noticeably warmer white point than the paper itself under the illuminant.
- Added support for the X-Rite i1Studio instrument. Note that you may have to un-install and re-install the system drivers on MSWindows, or update the udev 55-Argyll.rules file on Linux.
- Slight improvement to i1d3 accuracy, by rounding the frequency mode measurements up by 0.5.
- Returned input profile forced Absolute Colorimetric option with -ua flag, after the -u option was changed in V1.5.0.
- Try and fix problem in triggering calibration when ARGYLL_NOT_INTERACTIVE is set.
- Improve compatibility of txt2ti3, and added -D option to mark output as Display but not Normalized to white.
- Modified collink to disable Video encoded in/out sync level preservation.
- Added support for custom Observer by using a .cmf file as an argument to all tools taking an observer parameter.
- Added support for proposed CIE 2012 2 degree & 10 degree observers, based on the CIE (2006) 2-deg LMS cone fundamentals.
- Fix problem with dispwin -E option not being shown in usage, and only being applied when a calibration file is used.
- Added spotread -u option to display XYZ amd CIE 1976 Yuv values.
- Added XRGA conversion support to spec2cie, as well as better support in chartread and txt2ti3 for tracking XRGA standard and polarization filter use.
- Fix bug in spec2cie processing emissive .sp files.
- Fix problem with i1d3 running direct USB (i.e. Not via HID) on MSWin.
- Fixed bug in render/timage -p.
- Changed spotread ambient readings (CCT, CRI, TLCI) to show CCT delta E in 1960 Duv units and others in Delta E 2000.
- Added ARGYLL_UNTWIST_GAMUT_SURFACE environment variable, that enables extra gamut clip surface processing that may improve the smoothness of device links and B2A tables for poorly behaved devices.
- Fixed bug introduced in new colorimetric nearest clipping code in rspl/rev.c in V1.9.0 that caused colprof using some ink limit settings (such as -L0) to crash.
- Fixed bug introduced in new colorimetric nearest clipping code in rspl/rev.c in V1.9.0 that caused some (mainly XYZ clut) profiles to clip badly, causing banding.
- Improved dispcal -R VideoLUT depth measurement algorithm robustness.
- Worked around latest OS X super slow opening serial port problem (1.5 seconds to open a port!)
- Added ColorCheckerHalfPassport.cht file.
- Fixed bug in ChromeCast mDNS parsing that caused problems with some devices with long names being detected.
- Now ignoring Chromecast-Audio and (.ca flags & 1) == 0 devices, and showing the friendly chromecast name if available.
- Wait longer to find more Chromecasts, even if we've found one.
- Fixed colprof bug when handling Display L*a*b* .ti3 data.
- Added Wacom i1d3 support.
- Changed dispwin to by default ignore Gnome colord, and use its native ucmm for storage of display profiles, since colord support for ArgyllCMS has proven unreliable. This can be re-enabled by setting the ARGYLL_USE_COLORD environment variable (i.e. to "true").
- Change X11 root window _ICC_PROFILE_xxx atom setting for Xrandr case to now match the Xinerama order, so that ICC_PROFILE_xxx atoms match, irrespective of which extension applications are using. This improves conformance to "ICC Profiles in X Specification 0.2".
- Improved ucmm install/load/delete to better respect systemlocal/user scopes, as well as eliminating need for profile name on delete when ucmm is used.
- Improve fast serial port scan to better detect Lumagen Radiance without upsetting it.
- Added ARGYLL_EXCLUDE_SERIAL_SCAN environment variable, to allow suppression of fast serial port scan of sensitive devices.

# [V1.9.1 -> V1.9.2] 17th October 2016

- Added CMYKOGB and CMYKRGB 7 channel ink preset, and made targen more flexible in matching pre-conditioning profiles to targen ink selection.
- Fix oeminst for OS X save location.
- Fix oeminst for OS X Spyder 4 CD calibration file location.

# [V1.8.3 -> V1.9.1] 28th September 2016

- Improved robustness of ChromeCast discovery, and added some minimal diagnostics.
- Improved robustness of targen ofps patch generation when using less well behaved pre-conditioning profiles.
- Fixed oeminst so that it locates cdrom's in Linuxes latest mount point of /run/media/$USER/.
- Fixed bug in i1pro2 driver, in which strip calibration would fail if instrument had been first calibrated with ARGYLL_DISABLE_I1PRO2_DRIVER set, and then calibrated with ARGYLL_DISABLE_I1PRO2_DRIVER unset.
- Added option to icclib to write Output profiles using 'chad' tag if the ARGYLL_CREATE_DISPLAY_PROFILE_WITH_CHAD environment variable is set. This is not recommended for normal use, but may assist compatibility with other systems.
- Added JETI spectraval support, including Bluetooth access.
- Added support for the Klein K10 connecting via a serial port.
- Fixed bug in Colormunki Smile driver that causes crash on Ubuntu 16.04.1 LTS.
- Modified "lp" intent to greatly reduce eliminate Helmholtz-Kohlrausch appearance modelling.
- Fixed problem with targen -g, in that the corresponding XYZ values had double the power applied, rather than none. This was causing problems with printtarg spacer colors.
- Extensive re-write of colorimetric nearest clipping code in rspl/rev.c to restore precision that was lost in the speedups made in V1.0.0. The nnrev setup now takes a lot longer with high resolution CMYK profiles though. This corrects a "green becoming too yellow" problem for mapping from ProPhoto space with some RGB devices.
- Change dispwin to properly set X11 DirectColor and take account of TrueColor Colormap. This fixes problem with NVidia linux driver 364.12 exposing a VideoLUT depth that is different from the frame buffer depth.
- Change icclib to automatically repair icmTextDescription strings that have an allocation that is longer than their size.
- Added i1Pro Lamp Drift test and fix functions to spotread (-Y l|L options).
- Change colprof so that -s -S will accept general compression percentage as an alternative to a source colorspace/image gamut.
- Added optional conversion from native Gretag-MacBeth & X-Rite reflective calibration standards to/from XRGA.
- Changed OS X GUI support code so as not to switch to "interact with the Dock" mode until actual GUI element is to be displayed. This prevents batch commands with optional GUI elements from blocking normal GUI interactions.
- Re-jigged OS X UI code to use the main thread to avoid window creation timing issues and a warning backtrace on OS X 10.11.
- Added CMP_Digital_Target-7.cht
- Fix spec2cie to cope with .ti3 files that are missing device values, so that it can process a wider range of input CIE reference files.
- Changed implementation of ARGYLL_NOT_INTERACTIVE on MSWin to make it more reliable when operated progromatically.
- Fixed chartread so that if you are reading patch by patch, the location strings can be arbitrary (i.e. they don't have to conform to an alpha/num strip/patch pattern.)
- Added support for Sencore ColorPro V, IV & III colorimeters (based on Sequel Chroma colorimeter.).

# [V1.8.2 -> V1.8.3] 26th October 2015

- Added SpyderCheckr24 scaning .cht and .cie files.
- Fixed USB problem with i1pro (Rev B & D ?), where communications would occasionally break down on fast systems.
- Added another fixed display intergration time to i1pro non-adaptive emission mode to cope with higher brightness displays.
- Added workaround for i1d3 Rev. B status code 0x83 on very low light measurement
- Fixed minor bug in i1d3.c that truncated serial number string. (Thanks to Mikael Sterner).
- Fixed bug in Klein K10 driver - adaptive measurement wasn't properly using all the extra measurements.
- Improved Klein K10 driver to be more robust when lights off command returns bogus error codes, or causes a cascade of bogus measurement errors.
- Added workaround for OS X 10.9+ "App Nap" problem.
- Added maximum sensor frequency check for Spyder & i1d3 drivers, so that erronious readings due to excessive brightness can't be missed.
- Changed chartread so that it doesn't warn of a possible wrong strip being read, nor allows bi-directional strip reading, if "printtarg -r" was used. A warning will be issued if "printtarg -r" was used, and "chartread -B" wasn't used.
- Fixed collink for eeColor Full range RGB to use output curve ("second" 1D curves) to compensate for cLUT being wired for 1.0 output from 1.0 input.
- Added "lp" gamut mapping intent :- Luminance Preserving Perceptual, for Photographers concerned with maintaining tonal variations.
- Fixed bugs in image specific gamut mapping that were degrading the accuracy of the result.
- Re-wrote gamut smoothing code, and re-tuned it to behave similarly to the V1.8.2 release.
- Changed default viewing condition glare to 5%, to smooth out shadow tone curve.
- Reduced the level of Helmholtz-Kohlrausch effect in CIECAM02 implementation in the light of visual experiments.

# [V1.8.1 -> V1.8.2] 7th September 2015

- Fixed endless loop bug in alternate calibration selectors code.

# [V1.8.0 -> V1.8.1] 4th September 2015

- Fixed bug in "spec2cie -n" wrong field indexes were being used.
- Fixed colorimeter calibration selectors to add in alternate selectors if the letters are free.

# [V1.7.0 -> V1.8.0] 20th August 2015

- Added support for the Image Engineering EX1 spectroradiometer.
- Added support for the SwatchMate Cube reflective colorimeter, with improved accuracy.
- Added Added Television Lighting Consistency Index (EBU TLCI-2012 Qa) to spotread and specplot output.
- Added R9 value to CRI value in spotread and specplot output.
- Added workaround for JETI specbos having been calibrated by a 3rd party, and its calibrated range being out of sync with its claimed range.
- Added support for "EMISINPUT" type .ti3 file.
- Build using OpenSSL rather than axTLS if it is built on Linux.
- Fixed stack space problem in OS X UI programs by expanding main thread proxy to have 8MB instead of the default 512K.
- Updated built in libtiff to V4.0.4beta.
- Changed CGATS format to not emit unknown keyword declaration ("KEYWORD") by default.
- Added inst_calc_cond_mask to inst.h to allow for flags in calibration conditions. A consequence of this is that calc needs to be masked with this when comparing against a specific condition, and the inst_calc_optional_flag should be cleared if it is set, before callint inst->calibrate() if the user wants to proceed with a particular calibration.
- Fixed bug with dispcal -e N
- Fixed bug in xicclu -fg and -kp
- Added dispcal -x x option to allow reading a chart and manually entering the XYZ values.
- Fix spyder4 & 5 bug where some display types were set as refresh when they shouldn't be.
- Fix collink "Warning :- RGB black hack trigger more than once!" when -b is used with input video encoding (-e).
- Changed colprof so that the default ICC description is the base filename rather than the whole file path.
- Fix technology type and display type selector "uniqueification" bug that shows up in "ccxxmake -??".
- Add OEM field to ccmx and ccss files to mark files that have been installed from OEM disk, so that custom ccmx & ccss files can be given suggested selector letter priority (+ ref/CRT.ccss).
- Tweak CGATS write format to avoid scientific notation until the numbers are bigger and smaller (i.e until e6 and e-6 are needed).

# [V1.6.3 -> V1.7.0] 1st May 2015

- Improved gamut mapping to reduce unnecessary changes to less saturated colors such as skin tones.
- Add support for DataColor Spyder 5.
- Add support for ColorHug2 colorimeter.
- Add support for Klein K10-A colorimeter.
- Added Google ChromeCast as a test patch generator for Video displays.
- Added ls2ti3 tool to convert LightSpace .bcs files to .ti3.
- Added IRIDAS .cube 3DLut format support to collink.
- Add X3D and X3DOM support as an alternative to VRML, and make X3DOM the default.
- Add better cross compatibility with non-Argyll ICC profiles using ArgyllCMS 'arts' tag to mark 'wtpt' Absolute Colorimetric chromaticity transform, as well as implement proper absolute colorimetric intent for Display profiles use the 'chad' tag. Note that the standard ICC profiles provided by ArgyllCMS in the ref directory (such as sRGB etc.) now include an 'arts' tag.
- Ignore any patches that have zero values for creating Display profiles, unless they are for device zero.
- Fix various instrument communications problems for JETI specbos, DTP20, DTP92 & DTP94.
- Fix gestaltSystemVersion warning on OS X 10.10.
- Fix very major bug in illumread. It wasn't actually working at all since V1.4.0.
- Added collink -I[gG][:p.p]:x.x options that allows an output offset gamma curve be targetted instead of BT1886.
- Added dispcal and collink -b black point hack. This forces the input zero to map to the output zero for well behaved displays, reducing dependence on the instrument accuracy for a very dark black point.
- Added preset list of display techologies to select from in ccxxmake.
- Added a -P prune option to profcheck, that creates a .ti3 file pruned of any patches that have a delta E fit error greater than a threshold. This may be of use in eliminating bad reading values from a measurement set.
- Added histogram plot option -h to both profcheck and verify.
- Added a dispread & fakeread -Z option to set the number of bits to quantize the test values to.
- Fixed bug in targen - the -V dark emphasis wasn't being applied to OFPS generated points.
- Make sure that if an instrument display reading is interrupted by a forced calibration, that the user is asked to place it back on the display before resuming the measurements.

# [V1.6.2 -> V1.6.3] 26th January 2014

- Added ProPhoto.icm and ProPhotoLin.icm to ref profiles.
- Fix bug in xicclu -py conversion.
- Added code to minimize ICC rounding error on matrix profile white point accuracy. Re-generated all reference profiles with this change.
- Changed i1d3 driver to completely ignore any EEPROM checksum errors for non "A-01" rev. instruments.
- Made transplot handle RGB->RGB device link.
- Removed colprof -y option. Use "profcheck -v2" instead, as it is more developed.
- Fixed bug in dispcal - it was not using the final measurement pass to update the calibration curves.
- Fixed bug in spotread, dispcal & dispread for CCSS capable instruments where refresh display types was being ignored if a custom observer was used, and/or the custom observer as being ignored, and/or a CCMX was being ignored. Changed instlib semantics for inst_opt_set_ccss_obs :- this is now set immediately, and applied also to any subsequent set_disptype() or col_cal_spec_set().
- Renamed verify to colverify to avoid clash with MSWin program of the same name. Made it print the patch location for -v2 if it is present in the file.
- Changed targen to ensure that -V and -p options effects are reflected in the resulting expected CIE values of the .ti1 file.
- Changed targen so that -V parameter also affects single channel, grey wedge, grid & body centered grid point distribution.
- Changed colprof to deal with variable grid distribution in a more neuanced way, to reduce overshoot artifacts when the -V parameter is used.
- Changed colprof to used a power_like function for the grid distribution shape from the -V parameter, so as to avoid issues with a power curve infinte slope near zero.
- Changed colprof to used a scaled down value of the targen -V parameter as the default for its -V parameter. Documentation now recommends more moderate values for -V.
- Added a special case to collink for RGB video input encoding to (attempt) to fine tune the black point to compensate for it (probably) not falling on a cLUT grid point. & out encoding
- Tweaked dispcal to try and improve accuracy of black point calibration.
- Switch dispread to use NoClamp readings, so that average black point value is not biased.
- Fixed bug introduced into 1.6.2 oeminst that prevents .ccss files being installed.

# [V1.6.1 -> V1.6.2] 18th November 2013

- Added "dark region emphasis" -V parameter to targen and colprof, in an attempt to improve the accuracy of display profiles intended for use with video. This should improve the subsequent black point accuracy of the profile.
- Fixed bug and tweaked dispcal black point optimization to err on the black side. Added -v3 for even more debugging information.
- Changed i1d3 driver to be more forgiving of EEProm checksum calculation, so that it works with the latest release "A-02" rev. i1 display pro & colormunki display instruments, as well as improving its robustness in the face of errors.
- Fixed race condition bug in OS X HID driver. This fixes occassional problem with i1d3, and also solves problem with the ColorHug on OS X.
- Fixed problem with TV encoded output and dispread -E -k/-K.
- Fixed minor bug in DE94 in icclib.
- Fixed major bug in illumread - result was being corrupted.
- Fixed "edges don't match" bug in printarg when -iCM -h -s/-S used.
- Fix bug in -H flag in ccxxmake, chartread, dispcal, dispread, illumread & spotread so that it works once again.

# [V1.6.0 -> V1.6.1] 30th September 2013

- Fix bug in "average -m"
- Fix oeminst to work with a wider range of i1d3 install files.
- Fix ColorMunki reflective measurement accuracy, particularly for reflective readings. This has been poor since V1.5
- Fix bug in using DTP94 on Apple OS X introduced in V1.5
- Fix MadVR connect code to look for appropriate 32 bit or 64 bit .dll.
- Improve MSWin system driver installation by creating valid ArgyllCMS.cat file to match ArgyllCMS.inf. This eliminates the need to "Disable Driver Signature Enforcement", as well as allowing installation on MSWin 8.1.

# [V1.5.1 -> V1.6.0] 16th August 2013

- Added support for JETI specbos 1211 and 1201 (Thanks to JETI for their support!)
- Added Video profiling & 3dLut creation support for eeColor and MadVR. See video section in tutorial for pointers to relevant changes to tools. This includes support for MadTPG + various Video standard ICC profiles + verification workflow.
- Linux profile installation will use colord if libcolordcompat.so is present on system.
- Fix ColorHug driver so that it is backwards compatible with FW 1.1.8
- Made sure that MSWin test colors are not color managed. This may affect Vista, Win7 and Win8.
- Changed spectro/dispwin.c so that null transform color matching is used for displaying test patches on OS X >= 10.6. This should fix calibrating/profiling secondary displays on > OS X 10.6. Note that the 32 bit 10.4 binary will still have problems on > OS X 10.6.
- Changed instlib API ambient XYZ and spectral units to Lux. In previous versions of instlib they were Lux/pi.
- For those instruments that support it, made ambient readings honor refresh mode measurements, to improve repeatability when measuring regularly flickering light sources. (specbos, i1d3, i1disp).
- Changed spotread -ew mode to be Bradford chromatic transform rather than XYZ scaling, to better match Argyll ICC abs. vs. rel.
- Added support to xicclu to lookup colors though CAL files, both forward and backwards. Will also plot CAL file contents using -g.
- Added -Y R:rate option to spotread, dispcal, dispread & ccxxmake to allow setting a chosen display refresh rate. This can be used with the Colormunki display, as well as situations in which refresh rate measurement is not reliable.
- By default printtarg will create PS and EPS files with a CUPS job ticket to disable color management. Use the -U flag to disable this.
- Added display update delay calibration support to i1pro and ColorMunki (just like i1disp3), to improve measurement times.
- Changed dispcal & dispread so that they wait up to 0.5 seconds when reading dark patches after light ones to allow for display fall time. Added patch order optimization for display patch sets in targen to minimize the extra time.
- Changed dispwin daemon loader mode option from -E to -X. Added -E option to encode test patch colors in Video 16-235 range.
- Changed dispcal verify option from -E to -z. Added -E option to encode test patch colors in Video 16-235 range.
- Added -E option to to dispread to encode test patch colors in Video 16-235 range.
- Changed CIECAM02 Flare model to distinguish between Flare from the image itself, and Glare from ambient light. This allows scaling Glare with ambient automatically. Changed enumerated viewing conditions for new Flare/Glare settings, changed all to Flareless to improve dark image behavior, while retaining Glare modelling. Tweaked brightness and ambient values.
- Improved i1pro hi-res mode to improve accuracy.
- Added Body Centered Cubic grid option to targen.
- Added -Yn flag to dispcal and dispread, which skips asking the user to place the instrument on the measuring spot.
- Improve robustness of i1d3 display update measurement code.
- Added support for applying calibration curves in collink.
- Changed spotread so that it won't fall back to emissive spot mode if an ambient reading is requested.
- Turned off B2A table clip map smoothing, as it seems to introduce reversals for some data sets, and provides little benefit.
- Fixed crash in ucmm/ucmm.c when loading certain profiles using dispwin (thanks to Torok Edwin).
- Fixed gamut mapping intent "rl" to really use relative L*a*b*
- Fix bug in cicam02 in V1.5.0 that causes some mapping problems in the red for collink -ir or -ila.
- Changed cctiff so that it does lossless JPEG copy when there is no color transformation. This makes it more useful for embedding a profile.
- Fix xicclu so that it works with device links.
- Fixed bug in shaper/matrix profile curves that caused random bumpy black behaviour (shaper curve optimization local minimum problem).
- Don't add colorant tag to .tiff files in cctiff unless it is a non-standard space, as Photoshop will barf on such files.
- Fix bug with Spyder not being able to break out of dispcal adjustment loop.
- Fix bug in xicc/xicclu, -K flag not being recognised.
- Fix bug in xicc/xmatrix.c introduced in V1.5 that prevents matrix only profiles from being created.
- libusb 1.0 is now deprecated in favor of native USB drivers.

# [V1.5.0 -> V1.5.1] 8th March 2013

- Fix spectro/instlib.ksh and standalone instlib build.
- Turned off debug plot on using FWA.
- Changed link $(LINKFLAGS) location in link command line Jambase to get latest gcc working.
- Fixed new bug in matrix display profile creation that causes an inaccurate relative white point. This causes Photoshop to barf on the profiles.
- Added -m option to printcal.
- Fix bug in webwin that causes crash.

# [V1.4.0 -> V1.5.0] 1st March 2013

- Increased ease of selecting ISO 13655:2009 M0, M1 and M2 measurements using FWA comensation using any spectrometer that can take non-UV filtered measurements. M0, M1 or M2 can now be selected directly using the -f flag. [ArgyllCMS has been supporting ISO 13655 M0, M1 & M2 well before the standard was created, thanks to its FWA compensation feature.]
- Increased stability of i1d3 refresh display measurements by increasing integration time, and tweaking crossover from frequency to period measurement.
- Added i1pro Rev E (i1pro2) feature support. Uses RevE measurement mode, and does wavelength calibration. Uses RevE (internal) stray light reduction, and black level temperature compensation. The only Rev E feature not currently supported is U.V. measurement, which would improve the accuracy of FWA compensation. Rev E driver can be disabled and the legacy driver mode used by setting the ARGYLL_DISABLE_I1PRO2_DRIVER environment variable.
- Changed i1pro adaptive mode to avoid high gain mode, so as to give more consistent and longer integration times for low light levels.
- Changed ColorMunki adaptive mode to avoid high gain mode, so as to give more consistent and longer integration times for low levels. Added black level temperature compensation.
- Added spotread interactive function 'f' to read out the calibrate display refresh rate for instruments that have a refresh display mode, as well as an 'F' function that measures the refresh rate for instruments that support a refresh rate measurement function (colorimeters & spectrometers).
- The Display Type selection option -y in dispcal, dispread, chartread, spotread & ccxxmake now lists installed CCSS and CCMX files as a selection, rather than using the -X parameter. CCMX and CCSS files now have extra fields to indicate the refresh mode, an optional list of default UI selection characters, and (for CCMX files) the base display type they apply over (CB-n).
- Tweaked CIECAM02 to improve behavior for extreme blue colors, so that the hue doesn't swing too far towards the cyan. This helps in the clipping behavior from colorspaces such as ProPhotoRGB.
- Made the input profile cLUT extra neutral axis extrapolation points the default for colprof -u and non -u profiles. Changed -u algorithm to work similarly to -U scale :- it sets the scale automatically. Relative colorimetric is therefore hue matched to the white reference patch, Removed colprof -un, as it seems unnecessary. Added colprof -uc, which clips cLUT colors over Y = 1 to white.
- The spyd2en, spyd4en and i1d3ccss tools have been combined into, and replaced by a single oeminst tool.
- Fix problem with dispwin/dispcal/dispread -dweb and the latest Safari browser.
- Changed to a single ArgyllCMS.inf file for MSWin USB driver installation. This eases installation of more than a single type of instrument. Tested on MS Windows 8 and updated installation instructions.
- Dropped libusb for USB access, using native USB access instead. MSWin uses the libusb-win32 kernel driver. Moved the usb setup files from libusb1 to a new directory, usb.
- Added scanin support for ColorCheckerPassort.
- Updated OS X code to compile on 10.6 and 10.7 and (presumably) 10.8 (64 bit compatible API used when compiling on those platforms, including Cocoa for the test patch window).
- Changed udev file usb/55-Argyll.rules to eliminate the test for /lib/udev/udev-acl as a condition of using ACL_MANAGE, since I'm informed that it is deprecated in recent distribution releases (but who can tell, given the churn in the udev API).
- Deprecated -V flag (adaptive mode) in dispcal, dispread and ccxxmake, since this is now the default. Flag will be ignored with a warning. Added -ZA flag instead, to select non-adaptive integration time mode.
- spotread -d flag is deprecated, and is now a synonym for the -e flag, since it defaults to adaptive mode. Added -ZA flag instead, to select non-adaptive integration time mode. Also added -Zr and -ZR flags to allow testing of the refresh mode overrides.
- Migrated ArgyllCMS specific application runtime files (such as instrument blobs, calibration state & calibration files) to an "ArgyllCMS" sub-directory rather than the generic "color" directory. On OS X also moved data files to below the "Application Support" sub directory. The old locations will be used as a fallback.
- Added support for Quato Silver Haze 3 OEM i1d3
- Added support for X-Rite ColorMunki Smile colorimeter.
- Enable the ColorHug by default, although it isn't advertised as supported, since it doesn't yet work reliably on OS X. Updated ColorHug PCI VID & PID
- For Spyder, emit a warning rather than error if the feature bits are missing for calibration tables.
- Added automatic adjustment of patch reading delay for i1d3, so that a more conservative (longer) default value (200 msec) can be used without impacting i1d3 speed. Also added environment variable ARGYLL_MIN_DISPLAY_UPDATE_DELAY_MS that can set a different minimum update delay.
- Fixed a bug introduced in V1.3.6 that stops the dtp41 from being initialized properly.
- Improved black level readings derived from spectral values by allowing them to be -ve.
- The instlib API has been modified quite extensively to make it more self contained and flexible, although the basic architecture remains the same.

# [V1.3.7 -> V1.4.0] 20th April 2012

- Modified spectro/ccxxmake so that a colorimeter can be used as a reference to make ccmx files if two .ti3 files are used. Added ref/ccxx.ti1 as convenient way of creating ccmx .ti3 files.
- Added dither/screening support for 8 bit output of render, and then made it available in target/printtarg.
- Added JPEG file support to imdi/cctiff, xicc/tiffgamut and xicc/extracticc. ICC profiles embedded in JPEG files can now be used anywhere a TIFF file with embedded ICC profile can be used as a source of an ICC profile.
- Fixed memory leaks in usbio.c, xdg_bds.c & conv.c
- Fixed double memory free bug in icc/icc.c when iccdump'ing a profile that has a duplicate tag.
- Changed license of xicc/ccmx.[ch] to GPL2+.
- Made display calibration and profile making deal with displays without hardware calibration support (VideoLUT support) more graceful. Added tutorial section covering this.
- Added option to dispwin/dispcal/dispread/ccxxmake to redirect the test patches to a web browser via a local web server. This augments Argyll's existing local and remote display capability.
- Fixed bug in spectro/i1d3.c which results in NAN if a low level readings drops to zero at a particular time. Improved refresh rate calibration accuracy. Fixed bugs in adaptive measurement logic that caused a channel to be pre-measured when it shouldn't. This seems to noticeably improve repeatability on refresh displays.
- Fixed bug in ucmm/jcnf where it was failing to locate the correct profile for a display.
- Fix bugs in ColorMunki Transmissive measurement mode calibration.

# [V1.3.6 -> V1.3.7] 26th March 2012

- Fix regression in Spyder support - ccmx files were not being handled (bug introduced in 1.3.6).
- Fix packaging problem - Spyder4 MSWin .inf file was missing.
- Change dispwin so that it will install a profile when there is no access to the display VideoLUT if the profile has no vcgt.

# [V1.3.5 -> V1.3.6] 19th March 2012

- Added Spyder4 support. Note the need for spyd4en for access to a full range of Manufacturers calibrations. The Spyder4 can use .ccss calibration files too. Speeded up all Spyder instrument readings on brighter colors.
- Experimental ColorHug support is compiled in, but is disabled unless the environment variable "ENABLE_COLORHUG" is set. The ColorHug currently doesn't seem to work reliably across all platforms ArgyllCMS supports.
- Changed and expanded display selection (-y flag) to be instrument specific. This is to support the Spyder4 and ColorHug, and adds a refresh display selection to the i1d3.
- Tweaked i1d3 integration times and added accurate refresh period calibration to the refresh display mode. Refresh display measurement times are double non-refresh displays. Improved i1d3 period measurement logic to improve measurement speed and accuracy for dark colors.
- Changed i1disp measurement logic to try and make it more robust against light to dark changes during a reading. This may make it slightly less precise for LCD displays on bright colors (equivalent now to Refresh display precision).
- Added a -V option to spotread to allow tracking reading consistency.
- Changed ccxxmake to create default .ccss with just RGBW, and not to weight W. This may give better matching. Made corresponding change to CCMX, giving the white patch 1/4 weighting of sum of all other patches.
- Fixed applycal so that it applies calibration to both A2B and B2A tables, to preserve softproofing.
- Fixed timeout in SpectroScanT reference transmission measurement. (Someone kindly donated me a SpectroScanT to test with!)
- Made DTP94 driver ignore with a warning any NEEDS_OFFSET_DRIFT_CAL_ERR after a full reset. It seems that occasionally a few instruments do this, and X-Rite don't appear to be prepared to treat this as an instrument fault.
- Added support for Datacolor SpyderCheckr (Thanks to Jos Pereira).
- Improved the ability of spyd2en to cope with slightly different setup.exe formats.
- Add support for NEC SpectraSensor Pro version of the i1d3.

# [V1.3.4 -> V1.3.5] 24th October 2011

- Fix bug (crash) that affects ColorMunki design/photo display measurement. This also stops it restoring a calibration (-N flag).
- Add support for the OEM version of the i1d3.
- Fix bug that stopped ccxxmake being able to make ccmx's.
- Tweak gamut mapping to improve dark area mapping, non-monotonic profile inversion, and contrast preservation to small gamut.
- Kill i1ProfileTray.exe process if unable to open i1d3 on MSWin.
- Fix DTP20 chart printing - TID was sometimes incomplete. This shows up on a 4x6 chart.

# [V1.3.3 -> V1.3.4] 31st August 2011

- Added support for the X-Rite i1 Display Pro and ColorMunki Display colorimeters. As part of this, added support for CCSS calibration files for the instruments and added CCSS support to ccxxmake (renamed from ccmxmake). Provide new tool i1d3ccss to translating and installing CCSS files as well as the manufacturers calibration files for these instruments. Added non-default observer support for these instruments too.
- Fix gamut code to ignore setting primary/secondary cusps that are unlikely to be true. This avoids buggy gamut mapping behavior for gamuts that are very small and odd shaped.
- Changed Linux USB code to avoid doing a set_configuration if possible, since the USB driver does this by default. This then avoids triggering a bug in the Spyder2, which allows it to work on Linux version without the reset_ep fix, and may also allow the Spyder to work better with USB hubs.
- Change printtarg for DTP20 to allow for variable patch size.
- Changed dummy display matrix table to have channels rotated rather than R & G swapped, to make it more obvious.
- Added option to colprof to allow setting the default profile rendering intent.
- Enhanced spectro/fakeread so that it will process a .ti3 file that has been renamed to .ti1.
- Fix bug in matrix input profile white point selection, + add in slight neutral bias code used in clut profiles.
- New profcheck -I wasn't working - fix option parsing.

# [V1.3.2 -> V1.3.3] 13th May 2011

- Fixed compiler dependant bug in Eye-One pro and (possibly) Munki high res. spectral wavelength calculation.
- Add support for install variables DESTDIR and PREFIX in Jamtop. These can be set on the command line using "jam -s"
- Added targen -N parameter to allow adjustment of neutral axis patch density emphasis, as well as increasing the default. This should improve the result without needing to add explicit grey test patches.
- Added spectro/instlib.ksh script to assemble all the files needed for a standalone instrument library. Changed licence to GPLv2 for the files included in the instlib.zip file that is thus created. See spectro/instlib.txt for more details.
- Fix Jambase so that recent MingW compilers don't need extra .dll's
- Change Linux serial code to test ports using O_NONBLOCK
- Modify xspect & illumread to improve realism of UV spectrum estimation.
- Fixed profile/txt2ti3 so that a sample name that looks like an integer is treated as text. (Fixes problem with latest ProfileMaker file).
- Added LCh option to spotread.
- Fixed numerical issue in scanin/scanrd.c, where large input rasters would cause fitting to fail.
- Modified colprof input chart white patch detection to slightly favour patches that are close to D50 neutral.
- Increase the default XYZ PCS A2B profile default smoothness.
- Improved cLUT input -u black & white point extrapolation.
- Improved black point determination for devices that have extremely narrow gamuts doe to the use of custom inks.
- Added -Z option to colprof, to allow setting ICC attribute flags.
- Fix CIECAM02 to better match forward and backwards, to fix perceptual table white point.
- Add code to override X-Rite's new OS X drivers for ColorMunki and EyeOne. Note new installation instructions <http://www.argyllcms.com/doc/Installing_OSX.html>.
- Added -R flag to colprof, which restricts the range of the white, black for better compatibility with other programs.
- Fixed typo bug that prevented flash measurement mode from working.
- Replaced spectro/average with a new version that is more general.
- Fixed bug in printcal not working with spectral only files.
- Added extra verbose output to printcal in which it computes an ideal power-like value to apply to the test chart values in targen.
- Modify the way that XYZ cLUT B2A tables are indexed, so that the white point is at the top corner of the grid.This should solve Photoshop CS4/CS5 complaining that XYZ LUT profiles are 'defective'.
- Added option in xicc/xicclu to plot an arbitrary slice.
- Expand the number of i1 Display OEM devices that can be used.
- Made some changes to help compile on FreeBSD.
- Added another intent, "pa", Perceptual Appearance, which is the same as perceptual except that the grey axes are not forced into alignment, allowing the appearance parameters to have full affect, including altering the chromatic mapping.
- Fixed bug in txt2ti3 - it wasn't creating an iRGB colorspace file for output device RGB files, causing warnings warnings and failures when mixed with other iRGB tool sequences.
- Added pathological case fix for target/ofps where the ink limit == di-2.
- targen was failing to proceed when fixed points happened to be numerically just over the total ink limit.
- Added more navigation options for chartread patch by patch mode.
- Fixed bug in "chartread -r -H" that caused resume of i1Pro high res to fail with "The resumed spectral type seems to have changed".
- Modified profcheck so that it prints patch location if it is present in the .ti3 file.
- Changed dispcal and dispread -K option to -J. Added -K option to dispcal as an alternate way of profiling a calibrated display, and also added a -K option to dispcal.
- Increased ColorMunki emissive auto scaling target "over" margin from 5% to 10% to allow more room for instrument drift during measurement.
- Fix bug in winusb + i1Display, where dark CRT measurements timeout.

# [V1.3.1 -> V1.3.2] 4th November 2010

- Turn off debugging that was accidentally left on in FWA code. Add gcc 3.3 PPC optimizer bug workaround to FWA code in xicc/xspect.c
- Change shaper/matrix profile back to using power curve as 0th order shape. Improve it with input & output offsets and straight segment at zero. Make cLUT input -u black & white point extrapolation use pure shaper curves with special tweaks.
- Increase dispcal native white target weighting from 10 to 50 to encourage white to be device 1.0,1.0,1.0 more strongly.

# [V1.3.0 -> V1.3.1] 26th October 2010

- Fixed MSWIN Vista/Win7 problem where having Task Manager running would stop display test window updating. Also fixed plot library to avoid the same problem.
- Swapped dispwin -E and -D flags, to make -D debug consistent throughout tools.
- Changed the ARGYLL_NOT_INTERACTIVE mode so that all return and line feed characters are ignored, so that they can be used freely to flush stdin without triggering anything.
- Fixed endless loop problem with chartread -r -p on fully read chart.
- Added -S option to chartread, that suppresses wrong strip and unexpected value warnings.
- Fix dispcal and spotread so that color temperature takes into account any non-standard observer (ie. the color temperature is the closest point on the spectrum locus as determined by the chosen observers interpretation of the Plancian or daylight spectrum.)
- Fix bug in libusb1 triggered on systems that support bulk continuation (Linux)
- Added 1964_10c observer to spectro/dispcal, to better allow comparison to the default numbers.
- Added recognition for Huey built into Lenovo W series Laptops.
- Fixed chartread/dispsup/spotread etc. so that -N isn't fatal if the instrument doesn't support it.
- Fixed dispcal to disable black & white drift tracking during interactive adjustment.
- Added -s option to ccmxmake to allow the number of test patches to be set.

# [V1.2.0 -> V1.3.0] 8th September 2010

- Added option to dispcal and dispread that attempts to counteract instrument black drift and display white drift (-I option). This may help with instruments that haven't properly acclimatised to the measurement location, and LCD displays that also take some time to stabilise. The is a short discussion here.
- Added option to dispcal to allow specifying a non 1931 2 degree observer if a spectrometer is being used.
- Added new utility spectro/ccmxmake, which makes Colorimeter Correction Matrices for a particular Colorimeter + Display combination, using a Spectrometer as a reference. The resulting .ccmx file can then be used with spotread/dispcal/dispread (-X option) to improve the accuracy of the colorimeter on that particular display. See a discussion here and here.
- Fixed bug in spotread's handling of emissive measurements. If the XYZ was computed from spectral, it was using a D50 white instead of no white reference.
- Fixed bug in i1pro normal resolution wavelength calibration, introduced in V1.2.0.
- Changed libusb V1.0 name to libusb-1.0A, so as not to clash with any official but different libusb V1.0 installation. [This may necessitate re-installing device drivers on MSWin.]
- Added support for HP DreamColor version of the i1 display.
- Fix problem with ARGYLL_NOT_INTERACTIVE - reading from instruments was not actually possible, because polling for input was disabled.
- Adjust ColorMunki dark threshold to reduce misread reports. Add inconsistent data to debug output. Fix bug in adaptive mode - the integration time was sometimes too short. Set adaptive emissive target at 95% to allow a little more margin to saturation.
- Fix problem with ColorMunki reporting erroneous inconsistent measurement errors. This shows up on display calibration.
- Fix some minor compiler warnings.
- Added direction indicators to xy values in dispcal interactive monitor adjustments.
- Fix bug in CIECAM02 viewing condition settings :- the enumerated conditions after "mt" are displaced by 1. (ie. "mt" is really "pc", "mb" is "mt", "md" is "mb" etc.) Added option -c:sn for auto surround from the Lv parameter (-c:l).
- Add option to illumread to average several readings. Fixed bug in the way illumread displays available instruments.

# [V1.1.1 -> V1.2.0] 30 July 2010

- Re-worked gamut mapping to improve perceptual intent saturation levels, as well as improve highlight and shadow contrast. Added fine tuning to improve both smoothness and the precision with which the source is mapped to the destination.
- Added illumread, which allows measuring an illuminant and estimating its UV content, for better accuracy with FWA compensation.
- Use a modified/forked version of libusb V1.0, that supports Win2K (libusb0.sys) back end by default. Supports 64 but MSWin using a combination of WinUSB.sys and ptlibusb0.sys. [ The HCFR does not work on Win 64 bit though, due to its buggy USB implementation. ] NOTE that the included version of Libusb V1 has been carefully tested with all supported instruments on all supported platforms, and includes many bug fixes needed for correct functioning. While bug fixes have been fed upstream, not all have been adopted. In particular there is a nasty race condition that has not, and may never be fixed upstream, as well as missing critical functionality (clearep()).
- Modified colprof -p to allow different abstract profiles to be applied for each intent.
- Added -I option (imitation) to printcal, so that an existing devices response can be set as a target.
- Increase target/ofps.c vertex intersection retries from 10 to 40 to give it a better chance of working with difficult profiles.
- Fixed bug in plot that shows up on XP+, where the window isn't dismissed by the first keystroke, but only after it has been moved or resized.
- Changed CMYK black point to be natural, rather than the darkest point in the same direction and K only. This may wreck K only to black point matching, but it will stop printers with funny colored K ink from messing up the black point.
- Make Lacie Blue Eye colorimeter appear as an i1display.
- Improved i1pro matching to Original Manufacturers Driver (see doc/i1proDriver.html).
- Improved i1pro/ColorMunki patch recognition for better uniformity.
- Fixed bug in ColorMunki driver scan mode calibration when instrument is more sensitive than usual.
- Added EV calculation to spotread -a

# [V1.1.0 -> V1.1.1] 21 February 2010

- Renamed the following tools:
  cb2cgats -> cb2ti3
  kodak2cgats -> kodak2ti3
  logo2cgats -> txt2ti3
  splitcgats -> splitti3
  mpprof -> mppprof
- Modified black curve to make sure that smoothed curve meets target level at boundaries.
- Added -M option to printtarg, for the case where the TIFF file is to include the margin.
- Fixed several build bugs in imdi code related to 64 bits.
- Fixed profile/colprof -u so that it is applied to matrix profiles too
- Changed tiffgamut to use one pass gamut hull finding and modified the smoothing so as to end up with a more closely wrapped volume.
- Fixed bug in input matrix profiles introduced by the XYZ cLUT display matrix profile change, where the correct white and black point weren't being written.
- Added matrix only/linear algorithm option to profile/colprof, for raw camera profiling.
- Modified libusb/55-Argyll.rules for better compatibility with systems that have ACL installed but no ConsoleKit. Also set ID_VENDOR and ID_MODEL using. usb-db.
- Modified target/targen to cope better with case where adding nodes fails to determine vertex positions a lot of the time, causing extreme slowdown.
- Fixed colprof so that the per channel input curves for XYZ PCS B2A tables are actually scaled correctly.
- Changed link/collink to apply Y to L* curve if the input or output space is XYZ. Fixed the Y to L* scaling to make sure it only apples to XYZ space, and that the L* non-linearisation still applies to Y like device spaces.
- Modified scanin so that it ignores any alpha channels in the input .tiff file.
- Changed printcal so that it will create .AMP file with more than 4 channels. Also fixed up plotting to plot up to 10 channels.
- Changed dispcal and dispread so that a request for projector mode falls back to display mode if the instrument doesn't support a projector mode.
- Updated ref/CMP_Digital_Target-3.cht as it seems that the reference chart has columns labelled "2A - 2D" rather than the "AA - AD" that is actually printed on the chart...
- Altered xpsect FWA code to reduce overshoot artefacts due to filtering.

# [V1.0.4 -> V1.1.0] 17th January 2010

- Spyder3 and ColorMunki Design, Photo and Create instrument support.
- Added a complete printer calibration system. This can work either with a print system that supports per channel print calibration curves, or purely using ICC profiling mechanisms.
- Default targen (OFPS) test point distribution has been re-written to generate test points on the gamut surface, refine the point locations when using a guide profile, and use a better error estimate model to determine the test point locations.
- Changed chartread strip reading mode to allow navigating about the strips, saving a partially read chart, and resuming a partially read chart.
- Improved and re-tuned gamut mapping. This is noticeably smoother and better retains source image detail.
- Re-tuned the cLUT profile creation smoothness vs. accuracy.
- Fixed viewgam so that the number of gamuts that can be viewed is unlimited. Also added error when computing intersecting volume if the two gamuts are incompatible.
- Improved CMYK black generation control and smoothness near the black point.
- Improved collink special black and colorant handling so that the gamut mapping is consistent with the special black and colorant mapping
- Changed profile/colprof to generate matrix tags for Display XYZ PCS cLUT profiles, to improve compatibility with other CMMs.
  By default (-ax) the matrix tags will be a dummy transform that swaps red and green, while using -aX will create real matrix tags.
- Added -V option to dispcal and dispread to allow use of i1pro adaptive mode to give better low level consistency.
- Changed dispcal to default to -f 1.0 (assume black is all output offset) to make it work in more sympathy to a typical display response. Also changed default gamma to 2.4 for OS X 10.6 systems.
- Improved X11 XRandR CRTC detection.
- Added spotread option to save spectral reading of an illuminant to a .sp file.
- Added Color Rendering Index (Ra) to spotread measurement results.
- Added i1pro & ColorMunki flash measurement support.
- Improve reliability of detecting backwards read i1pro/Munki strips.
- Fixed bug in i1pro driver that subtly affected accuracy.
- Modified xicc/cam02 to clip the blue to avoid crazy behavior outside the spectrum locus.
- Simplified the Linux installation instructions, particularly with regard to USB and serial permissions.
- Added working MSWindows 64 bit libusb drivers, which will work on Vista 64 and MSWindows 7 64 bit. Because of Microsoft's driver signing requirements though, they won't be usable unless a driver code signing workaround is used.
- Changed printtarg so that the TIFF output has the paper margin subtracted from it. This is so that the resulting TIFF can be placed on that sized paper without clipping or scaling. Set the margin to zero to get a TIFF that exactly fits into the specified paper size

# [V1.0.3 -> V1.0.4] 30th June 2009

- Modify icc/icclib to protect against integer overflow exploits, and fixes to minor bugs. Bump icclib version to 2.11 to reflect this.
- Fix bug in spectro/hidio.c that can cause a crash (bus error) on OS X for any program that accesses the instruments.
- Fix bug in xicc/xfit.c where too little memory was being allocated.

# [V1.0.2 -> V1.0.3] 3rd September 2008

- Added multi-TIFF and popularity filtering to tiffgamut.
- Modified gamut mapping in colprof and collink to be consistent, and have higher perceptual intent saturation.
- Fixed timeout problem with the Eye-One Display colorimeter.
- Fix segmentation fault in dispread.
- Fix out of memory error in colprof for systems with > 3Gig Ram.
- Add support for the Eye-One Monitor spectrometer.
- Added -L option to printtarg to suppress the i1pro target holder clip margin.
- Fixed bug in dispcal when using -a with -t

# [V1.0.1 -> V1.0.2] 19th August 2008

Various bug fixes, the main ones being:

- Fixed some colprof performance and memory usage issues.
- Fixed issues with Eye-One Pro Rev B timeouts.
- Added new option to collink -fk, that forces 000K input to K only output.
- Added device target value quantization option to printtarg, as well as making it default for TIFF output files.put files.
- Fixed leak that was affecting printtarg.

# [V0.70 Beta 8 -> V1.0.0] 1st July 2008

Apart from numerous bug fixes and many minor feature additions and improvements, the main changes to this version compared to the previous one are:

- Speedup in profile and device link generation (inversion code), and better memory usage.
- Support for embedded profiles in TIFF files.
- Support for installing and uninstalling and loading of display profiles for all operating systems, and a micro CMM system for X11/Linux
- Improved display calibration and profiling, including ambient light adjustment.
- X11 XRandR 1.2 support added.
- Raster test charts now supported, as well as PS and EPS.
- Guidance for installing on a wider range of systems.
- Fixed luminance and ambient calibration issues with various instruments.
- Renamed "profile" to "colprof", and "icclink" to "collink" to avoid clashes that have arisen with other executable names.
- Streamlined source code build system, for much easier building.
- Installation archives now include a top directory, and gzip/tar format for OS X and Linux.
- Added B2A table to input device LUT profiles by default.

As usual, a more detailed description of all changes is in the log.txt file that accompanies the source code.

# [V0.60 -> V0.70 Beta 8]15th January 2008

- Added quick display ICC profile creation as part of calibration.
- Added support for the Huey, Spyder 2, DTP20, Eye-One Pro, DTP22/Digital Swatchbook, Eye-One Display 1 and 2 instruments.
- Changed to GPL Version 3 license.
- Countless other bug fixes and feature enhancements.